# Software Information
display_name = "The 3DO Company - 3DO (4DO)"
authors = "JohnnyDude|FreeDO team|trapexit"
supported_extensions = "iso|bin|chd|cue"
corename = "4DO"
categories = "Emulator"
license = "LGPL/Non-commercial"
permissions = ""
display_version = "v1.3.2.4+"

# Hardware Information
manufacturer = "Panasonic|GoldStar|Sanyo"
systemname = "3DO"
systemid = "3do"

# Libretro Features
database = "The 3DO Company - 3DO"
supports_no_game = "false"
savestate = "true"
savestate_features = "basic"
cheats = "false"
input_descriptors = "true"
memory_descriptors = "false"
libretro_saves = "true"
core_options = "true"
load_subsystem = "false"
hw_render = "false"
needs_fullpath = "true"
disk_control = "false"
is_experimental = "false"

# BIOS/Firmware
firmware_count = 10

firmware0_desc = "panafz1.bin (Panasonic FZ-1 BIOS)"
firmware0_path = "panafz1.bin"
firmware0_opt = "true"

firmware1_desc = "panafz10.bin (Panasonic FZ-10 BIOS)"
firmware1_path = "panafz10.bin"
firmware1_opt = "true"

firmware2_desc = "panafz10-patched.bin (Panasonic FZ-10 BIOS [RSA Patch])"
firmware2_path = "panafz10-patched.bin"
firmware2_opt = "true"

firmware3_desc = "panafz10e-anvil.bin (Panasonic FZ-10E BIOS [Anvil])"
firmware3_path = "panafz10e-anvil.bin"
firmware3_opt = "true"

firmware4_desc = "panafz10e-anvil-patched.bin (Panasonic FZ-10E BIOS [Anvil RSA Patch])"
firmware4_path = "panafz10e-anvil-patched.bin"
firmware4_opt = "true"

firmware5_desc = "goldstar.bin (Goldstar GDO-101M BIOS)"
firmware5_path = "goldstar.bin"
firmware5_opt = "true"

firmware6_desc = "sanyotry.bin (Sanyo Try IMP-21J BIOS)"
firmware6_path = "sanyotry.bin"
firmware6_opt = "true"

firmware7_desc = "3do_arcade_saot.bin (Shootout At Old Tucson BIOS)"
firmware7_path = "3do_arcade_saot.bin"
firmware7_opt = "true"

firmware8_desc = "panafz1-kanji.bin (Panasonic FZ-1 Kanji Font ROM)"
firmware8_path = "panafz1-kanji.bin"
firmware8_opt = "true"

firmware9_desc = "panafz10ja-anvil-kanji.bin (Panasonic FZ-10JA Kanji Font ROM)"
firmware9_path = "panafz10ja-anvil-kanji.bin"
firmware9_opt = "true"

notes = "(!) panafz1.bin (md5): f47264dd47fe30f73ab3c010015c155b|(!) panafz10.bin (md5): 51f2f43ae2f3508a14d9f56597e2d3ce|(!) panafz10-patched.bin (md5): 1477bda80dc33731a65468c1f5bcbee9|(!) panafz10e-anvil.bin (md5): a48e6746bd7edec0f40cff078f0bb19f|(!) panafz10e-anvil-patched.bin (md5): cf11bbb5a16d7af9875cca9de9a15e09|(!) goldstar.bin (md5): 8639fd5e549bd6238cfee79e3e749114|(!) sanyotry.bin (md5): 35fa1a1ebaaeea286dc5cd15487c13ea|(!) 3do_arcade_saot.bin (md5): 8970fc987ab89a7f64da9f8a8c4333ff|(!) panafz1-kanji.bin (md5): b8dc97f778a6245c58e064b0312e8281|(!) panafz10ja-anvil-kanji.bin (md5): 428577250f43edc902ea239c50d2240d"

description = "A port of 4DO, itself a fork of FreeDO, to libretro. One of several BIOS ROMs must be placed into your RetroArch / libretro "System Directory" folder. "norsa" versions have the RSA encryption check disabled which should allow unsigned software to run. This core is very demanding and is still in development, so many games have varying levels of compatibility and/or bugs."
